[**Air Sampling Pumps**](https://www.skcltd.com/products2/air-sampling-pumps.html) **and** [**Kits**](https://www.skcltd.com/air-sampling-kits.html)

SKC offers a wide range of pumps for all your air sampling and workplace air monitoring needs. Whether you are sampling for dusts/particulates, vapours/gases, bioaerosols or environmental, high or low flow rates, and whatever your environment we have a sample pump suitable for you. See our [Sample Pump Selection Guide](https://www.skcltd.com/knowledge-library/product-selection-guides/air-sampling-pumps-selection-guide.html) for more advice. Below is a selection of our pumps please see website for information on our complete range.

[**Sidekick**](https://www.skcltd.com/products2/air-sampling-pumps/sidekick-pump.html) **Dust & Vapours**

* Simple to use - ATEX and UKEX certified models
* Flow Range: 5 to 3000ml/min

[**AirChek 3000**](https://www.skcltd.com/products2/air-sampling-pumps/airchek-3000-pump.html) **Dust & Vapours**

* ATEX, UKEX & IECEx Certified Ex/M1/EPL Ma Mine Certified
* Programmable
* Flow Range: 5 to 3250ml/min

**AirChek** [**Essential**](https://www.skcltd.com/products2/air-sampling-pumps/airchek-essential-pump.html) **and** [**Essential+**](https://www.skcltd.com/products2/air-sampling-pumps/airchek-essential-plus-pump.html) **Dust & Vapours**

* Touch Screen - Up to 40 hours run time
* Flow Range: 5 to 5000ml/min

[**AirChek Touch**](https://www.skcltd.com/products2/air-sampling-pumps/airchek-touch.html) **Dust & Vapours** [**AirChek Connect**](https://www.skcltd.com/products2/air-sampling-pumps/airchek-connect-pump.html) **Dust & Vapours**

* Touch screens - Programmable
* Flow range: 5 to 5000ml/min

[**Universal Pump**](https://www.skcltd.com/products2/air-sampling-pumps/universal-pump.html) **Dust & Vapours**

* Built-in flow indicator
* ATEX & UKEX certified models
* Exhaust port for bag sampling -Flow range: 5 to 4000ml/min

[**Pocket Pump Touch**](https://www.skcltd.com/products2/air-sampling-pumps/pocket-pump-touch-pump.html) **Vapours**

* Touch screen
* ATEX/UL approved -Flow range: 20 to 500ml/min

[**Leland Legacy**](https://www.skcltd.com/products2/air-sampling-pumps/leland-legacy-pump.html) **Environmental. Bioaerosol.**

* Ambient monitoring for dusts, bioaerosols or pesticides
* Up to 24 hour run time -Flow range: 5000 to 15000ml/min

[**Biolite+**](https://www.skcltd.com/products2/air-sampling-pumps/biolite-plus-pump.html) **Bioaerosol**

* Specifically designed for sampling biological hazards
* Flow range: 0 to 62L/min